1. Disconnect the back-up light switch connector (A).

1. Check for continuity between the No. 1 and No. 2 terminals of the back-up light switch 2P connector. There should be continuity when the shift lever is in reverse.

1. If necessary, replace the back-up light switch. Apply liquid gasket (P/N 08C70-K0234M) to the switch threads, and install the switch on the transmission housing. Tighten the back-up light switch to the specified torque.

1. Install the resonator chamber.

1. Install the battery base, then install the ground cable.

1. Install the air cleaner housing.

1. Install the battery. Connect the positive (+) cable first, then the negative (−) cable to the battery.

1. Enter the anti-theft codes for the audio and navigation system, then enter the customer's audio presets.

1. Do the power window control unit reset procedure.