Connecting rod

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Connecting rod | Pin-to-rod clearance |  | 0.012−0.025 mm (0.0005−0.0010 in.) | 0.035 mm (0.0014 in.)
Small-end bore diameter |  | 30.012−30.020 mm (1.1816−1.1890 in.) | ———
Large-end bore diameter |  | 53.0 mm (2.09 in.) | ———
End play installed on crankshaft |  | 0.15−0.30 mm (0.006−0.012 in.) | 0.40 mm (0.016 in.)