DTC 87-32: Side Airbag Cutoff Indicator Stays ON

1. Erase the DTC memory.

1. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off.

Does the SRS indicator stay on?

YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failure.

1. Turn the ignition switch OFF. Make sure nothing is on the front passenger's seat.

1. Disconnect the OPDS unit harness 8P connector (A) from the OPDS unit.

1. Turn the ignition switch ON (II).