1. Remove the four bolts, then remove the alternator oil shield (A) and alternator (B).

1. Install the alternator in the reverse order of removal.

1. Connect the positive cable to the battery first, then connect the negative cable.

1. Enter the anti-theft code for the radio and navigation system, then enter the customer's radio station presets.

1. Set the clock.

1. Do the power window control unit reset procedure.