1. Remove the oil jet, and inspect it as follows.
   - Make sure that a 1.7 mm (0.07 in.) diameter drill will go through the nozzle hole (A) (1.8 mm (0.07 in.) diameter).
   - Insert the other end of a 3.1 mm (0.12 in.) drill into the oil intake (3.2 mm (0.13 in.) diameter). Make sure the check ball (B) moves smoothly and has a stroke of about 2.0 mm (0.08 in.).
   - Check the oil jet operation with an air nozzle. It should take at least 120 kPa (1.2 kgf/cm 2 , 17 psi) to unseat the check ball.
   NOTE: Replace the oil jet assembly, if the nozzle is damaged or bent.

1. Carefully install the oil jet. The mounting torque is critical.

   Specified Torque: | 22 N·m (2.2 kgf·m, 16 lbf·ft)