Pedal Height

1. Turn the brake pedal position switch (A) counterclockwise, and pull it back until it is no longer touching the brake pedal.

1. Lift up the carpet. At the insulator cutout, measure the pedal height (B) from the left side of the pedal pad (C).

   Standard pedal height (with carpet removed):
   | LHD model:
   |  | M/T: | 144 mm (5.67 in.)
   |  | A/T: | 148 mm (5.83 in.)
   | RHD model:
   |  | M/T: | 134 mm (5.28 in.)
   |  | A/T: | 138 mm (5.43 in.)