Intermediate Shaft Reassembly

Exploded View Special Tools Required Driver 07749-0010000 Attachment, 52 x 55 mm
07746-0010400
Attachment, 35 mm I.D.
07746-0030400
Oil seal driver
07GAD-PH70201
NOTE: Refer to the Exploded View as needed during this procedure.

1. Clean the disassembled parts with solvent, and dry them with compressed air. Do not wash the rubber parts with solvent.

1. Press the intermediate shaft bearing (A) into the bearing support (B) using the special tools and a press.

1. Install, then seat the internal snap ring in the groove of the bearing support.

1. Press the intermediate shaft (A) into the shaft bearing (B) using the special tool and a press.

1. Install, then seat the external snap ring (A) in the groove of the intermediate shaft (B).

1. Install the outer seal (A) into the bearing support (B) using the special tool and a press.

1. Install the set ring.