A/T Countershaft Reverse Selector Hub and 3rd Gear Removal

Special Tools Required Bearing separator 07KAF-PS30200

1. Install the special tool on the 4th gear (A). Set a press on the countershaft (B) with putting a spacer (C) between the press and countershaft, and remove the reverse selector hub (D).
   NOTE: Some reverse selector hubs are not press-fitted, and can be removed without using the special tool and a press.

1. Remove the needle bearing, set ring, 35 x 47 x 7.8 mm collar, and cotters.

1. Set the press on the countershaft (A) with putting a spacer (B) between the press and countershaft, and remove the 3rd gear (C).

1. Remove the 37 x 41 x 82.8 mm collar, 5th gear, 1st gear, and 2nd gear.