1. Install the reverse lockout solenoid.

1. Connect the reverse lockout solenoid connector, back-up light switch connector, and mainshaft speed sensor connector.

1. Install the cable bracket, select cable, and shift cable.

1. Install the battery base.

1. Install the air cleaner housing.

1. Install the battery. Connect the positive (+) cable first, then the negative (−) cable to the battery.

1. Enter the anti-theft code for the radio and navigation system, then enter the customer's radio station presets.

1. Perform the power window control unit reset procedure.