1. Refill the transmission fluid from the oil filler plug hole of transmission, and until the transmission fluid overflows from the oil check bolt hole (A).

1. After it stops overflowing, install the oil check bolt (B) with a new washer (C).
   Fluid Capacity

   2.2 L (2.3 US qt, 1.9 Imp qt) at Fluid Change
   2.5 L (2.6 US qt, 2.2 Imp qt) at Overhaul

   Always use Honda Manual Transmission Fluid (MTF). Using motor oil can cause stiffer shifting because it does not contain the proper additives.