1. Turn the stabilizer bar (A) toward the front of the vehicle.

1. Move the steering gearbox to the driver's side, and rotate it so the pinion shaft points toward the front of the vehicle.

1. Carefully move the steering gearbox as an assembly toward the driver's side of the vehicle until the pinion shaft (B) clears the wheelwell opening. Be careful not to damage the brake lines with the pinion shaft.