VTEC Rocker Arm Test

Special Tools Required Valve inspection set 07LAJ-PR30102 VTEC air adapter 07ZAJ-PNA0101
VTEC air stopper
07ZAJ-PNA0200
Air joint adapter
07ZAJ-PNA0300
K20A6 Engine

1. Start the engine and let it run for 5 minutes, then turn OFF the ignition switch.

1. Remove the cylinder head cover.

1. Set the No. 1 piston at top dead center (TDC).

1. Verify that the intake primary rocker arm (A) moves independently of the intake secondary rocker arm (B).
   - If the intake primary rocker arm does not move, remove the primary and secondary rocker arms as an assembly and check that the pistons in the secondary and primary rocker arms move smoothly. If any rocker arm needs replacing, replace the primary and secondary rocker arms as an assembly, and test.
   - If the intake primary rocker arm moves freely, go to Step 5 .

1. Repeat Step 4 on the remaining intake primary rocker arms with each piston at TDC. When all the primary rocker arms pass the test, go to Step 6 .

1. Check that the air pressure on the shop air compressor gauge indicates over 400 kPa (4.0 kgf/cm 2 , 57 psi).

1. Inspect the valve clearance.

1. Remove the sealing bolt (A) from the relief hole, and install the VTEC air stopper (B).

1. Remove the No. 2 and No. 3 camshaft holder bolts, and install the VTEC air adapters (C) finger-tight.

1. Connect the air joint adapter (D) and valve inspection set (E).

1. Loosen the valve on the regulator, and apply the specified air pressure.

   Specified Air Pressure:
   290 kPa (3.0 kgf/cm 2 , 42 psi)

   NOTE: If the synchronizing piston does not move after applying air pressure; move the primary or secondary rocker arm up and down manually by rotating the crankshaft clockwise.

1. With the specified air pressure applied, move the intake primary rocker arm (A) for the No. 1 cylinder. The primary rocker arm and secondary rocker arm (B) should move together.
   - If the intake secondary rocker arm does not move, remove the primary and secondary rocker arms as an assembly and check that the pistons in the primary and secondary rocker arms move smoothly. If any rocker arm needs replacing, replace the primary and secondary rocker arms as an assembly, and test.

1. Remove the special tools.

1. Tighten the camshaft holder mounting bolts to 22 N·m (2.2 kgf·m, 16 lbf·ft).

1. Tighten the sealing bolt to 20 N·m (2.0 kgf·m, 14 lbf·ft).

1. Install the cylinder head cover.

K24A3 Engine

1. Start the engine and let it run for 5 minutes, then turn OFF the ignition switch.

1. Remove the cylinder head cover.

1. Set the No. 1 piston at TDC.

1. Move the secondary rocker arm (A) for No. 1 cylinder. The secondary rocker arm should move independently of the mid rocker arm (B).
   - If the secondary rocker arm does not move, remove the mid, primary, and secondary rocker arms as an assembly, and check that the pistons in the rocker arms move smoothly. If any rocker arm needs replacing, replace the mid, primary, and secondary rocker arms as an assembly, and test.
   - If the secondary rocker arm moves freely, go to Step 5 .

1. Repeat Step 4 on the remaining secondary rocker arms with each piston at TDC. When all the secondary rocker arms pass the test, go to Step 6 .

1. Check that the air pressure on the shop air compressor gauge indicates over 400 kPa (4.0 kgf/cm 2 , 57 psi).

1. Inspect the valve clearance.

1. Remove the sealing bolt (A) from the relief hole, and install the VTEC air stopper (B).

1. Remove the No. 3 camshaft holder bolts, and install the VTEC air adapters (C) finger-tight.

1. Connect the air joint adapter (D) and valve inspection set (E).

1. Loosen the valve on the regulator, and apply the specified air pressure.

   Specified Air Pressure:
   290 kPa (3.0 kgf/cm 2 , 42 psi)

   NOTE: If the synchronizing piston does not move after applying air pressure; move the rocker arm up and down manually by rotating the crankshaft.

1. With the specified air pressure applied, move the secondary rocker arm (A) for the No. 1 cylinder. The mid rocker arm (B), primary rocker arm (C), and secondary rocker arm should move together.
   - If the mid and primary rocker arms do not move together with the secondary rocker arm, remove the mid, primary, and secondary rocker arms as an assembly, and check that the pistons in the rocker arms move smoothly. If any rocker arm needs replacing, replace the mid, primary, and secondary rocker arms as an assembly, and retest.

1. Remove the special tools.

1. Tighten the camshaft holder mounting bolts to 22 N·m (2.2 kgf·m, 16 lbf·ft).

1. Tighten the sealing bolt to 20 N·m (2.0 kgf·m, 14 lbf·ft).

1. Install the cylinder head cover.