SRS components are located in this area. Review the SRS component locations LHD, SRS component locations RHD and the precautions and procedures before performing repairs or service. NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the body and related parts.

1. Remove these items from the left side of the vehicle:
   - Front door sill trim
   - Rear door sill trim
   - Center pillar lower trim

   - | Without side curtain airbag
   - | With side curtain airbag

   - Rear seat cushion
   - Trunk lid trim
   - Trunk rear trim panel

   - | Without trunk side spacer
   - | With trunk side spacer

   - Trunk side trim panel, left side

   - | Without trunk side spacer
   - | With trunk side spacer

   - Trunk lid hinge cover

1. Pull the carpet back as needed.

1. Disconnect the trunk lid opener/fuel fill door opener cable (A) from the opener (B)

1. LHD: Release the opener cable from the clip (C). Remove the cushion tape (E).
   RHD: Release the opener cable from the clips (C, D). Remove the cushion tape (E).

LHD
RHD