ATF pressure

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
ATF pressure | Line pressure (K20Z2 engine model) | At 2,000 rpm (min −1 ) (in P or N position) | 900−960 kPa (9.2−9.8 kgf/cm 2 , 130−140 psi) | 850 kPa (8.7 kgf/cm 2 , 120 psi)
1st clutch pressure (K20Z2 engine model) | At 2,000 rpm (min −1 ) (in 1st gear in M position) | 890−970 kPa (9.1−9.9 kgf/cm 2 , 130−140 psi) | 840 kPa (8.6 kgf/cm 2 , 120 psi)
2nd clutch pressure (K20Z2 engine model) | At 2,000 rpm (min −1 ) (in 2nd gear in M position) | 890−970 kPa (9.1−9.9 kgf/cm 2 , 130−140 psi) | 840 kPa (8.6 kgf/cm 2 , 120 psi)
3rd clutch pressure (K20Z2 engine model) | At 2,000 rpm (min −1 ) (in 3rd gear in M position) | 890−970 kPa (9.1−9.9 kgf/cm 2 , 130−140 psi) | 840 kPa (8.6 kgf/cm 2 , 120 psi)
4th clutch pressure (K20Z2 engine model) | At 2,000 rpm (min −1 ) (in 4th gear in M position) | 890−970 kPa (9.1−9.9 kgf/cm 2 , 130−140 psi) | 840 kPa (8.6 kgf/cm 2 , 120 psi)
5th clutch pressure (K20Z2 engine model) | At 2,000 rpm (min −1 ) (in 5th gear in M position) | 890−970 kPa (9.1−9.9 kgf/cm 2 , 130−140 psi) | 840 kPa (8.6 kgf/cm 2 , 120 psi)
Line pressure (K24A3 engine model) | At 2,000 rpm (min −1 ) (in P or N position) | 927−985.6 kPa (9.45−10.05 kgf/cm 2 , 134−142.9 psi) | 878 kPa (8.95 kgf/cm 2 , 127 psi)
1st clutch pressure (K24A3 engine model) | At 2,000 rpm (min −1 ) (in 1st gear in M position) | 917−995.4 kPa (9.35−10.15 kgf/cm 2 , 133−144.3 psi) | 868 kPa (8.85 kgf/cm 2 , 126 psi)
2nd clutch pressure (K24A3 engine model) | At 2,000 rpm (min −1 ) (in 2nd gear in M position) | 917−995.4 kPa (9.35−10.15 kgf/cm 2 , 133−144.3 psi) | 868 kPa (8.85 kgf/cm 2 , 126 psi)
3rd clutch pressure (K24A3 engine model) | At 2,000 rpm (min −1 ) (in 3rd gear in M position) | 917−995.4 kPa (9.35−10.15 kgf/cm 2 , 133−144.3 psi) | 868 kPa (8.85 kgf/cm 2 , 126 psi)
4th clutch pressure (K24A3 engine model) | At 2,000 rpm (min −1 ) (in 4th gear in M position) | 917−995.4 kPa (9.35−10.15 kgf/cm 2 , 133−144.3 psi) | 868 kPa (8.85 kgf/cm 2 , 126 psi)
5th clutch pressure (K24A3 engine model) | At 2,000 rpm (min −1 ) (in 5th gear in M position) | 917−995.4 kPa (9.35−10.15 kgf/cm 2 , 133−144.3 psi) | 868 kPa (8.85 kgf/cm 2 , 126 psi)