DTC Troubleshooting: 51, 52

DTC 51: Motor Lock DTC 52: Motor Stuck OFF

1. Check the No. 17 (30 A) fuse in the under-hood fuse/relay box.

Is the fuse OK?

YES | - | Reinstall the fuse, and go to Step 2 .
NO | - | Replace the fuse, and recheck.■

1. Disconnect the ABS control unit 25P connector.

1. Measure the voltage between the ABS control unit 25P connector terminal No. 9 and body ground.

Is there battery voltage?

YES | - | Go to Step 4 .
NO | - | Repair open in the wire between the No. 17 (30 A) fuse and the ABS modulator-control unit.■

1. Check for continuity between the ABS control unit 25P connector terminal No. 25 and body ground.

Is there continuity?

YES | - | Go to Step 5 .
NO | - | Repair open in the wire between the ABS modulator-control unit and body ground (G203).■

1. Reconnect the ABS control unit 25P connector.

1. Clear the DTC using the HDS.

1. Disconnect the HDS from the 16P DLC.

1. Turn the ignition switch OFF, then turn it ON (II) again.

1. Test-drive the vehicle at 15 km/h (10 mph) or more.

Does the ABS indicator come on, and is DTC 51 or 52 indicated?

YES | - | Replace the ABS modulator-control unit. ■
NO | - | The system is OK at this time.■