1. Install the seat in the reverse order of removal, and note these items:
   - Apply liquid thread lock to the front seat mounting bolts before reinstallation.
   - Make sure each connector is plugged in properly.
   - Manual seat: When tightening the seat mounting bolts, make sure the recline adjusters and seat tracks were locked securely.
   - Tighten the seat mounting bolts to the specified torque in the sequence shown, slide the seat all the way back and tighten (1) and (2), then slide it forward and tighten (3) and (4).
   - If equipped with a side airbag, reconnect the negative cable to the battery.
   - Reset the clock.
   - Perform the power window control unit reset procedure.