1. Check for continuity between the No. 17 terminal of power tailgate control unit connector A (26P) and body ground.

Is there continuity?

YES | - | Go to Step 15 .
NO | - | Go to Step 10 .

1. By using the screwdriver, close the latch in the tailgate.

1. Connect battery positive (+) terminal to the No. 26 terminal of power tailgate control unit connector A (26P), and connect negative (−) terminal to No. 13 terminal of one. Then, move the motor to closing direction less than one second.