Inspection

1. Install the 10 mm flange nut on the top of the damper rod.

1. Push on the damper by hand as shown.

1. Check for smooth operation through a full stroke, both compression and extension. The damper should extend in a smooth, continuous motion when the compression is released. If it does not (no compression or no extension), the gas is leaking, and the damper should be replaced.

1. Check for oil leaks, abnormal noises, or binding during these tests.