1. Attach the upper rubber dam (A), lower side rubber dam (B), clips (C), dashboard seal A (D), and dashboard seal B (E) with adhesive tape to the inside face of the windshield (F) as shown:
   - Be sure the rubber dam and clips line up with the alignment marks (G).
   - Be sure the dashboard seals line up with the lower side rubber dam.
   - Be careful not to touch the windshield where adhesive will be applied.

   Rubber dams adhesive tape:
   | Thickness 0.16 mm (0.0063 in.) Width 3.5 mm (0.14 in.)
   Clips adhesive tape:
   | Thickness 0.4 mm (0.016 in.) Width 10 mm (0.39 in.)
   Dashboard seal A adhesive tape:
   | Width 21 mm (0.83 in.)
   Dashboard seal B adhesive tape:
   | Width 12 mm (0.47 in.)