Perform this operation in a safe area.

NOTE: Perform brake linings surface break-in when replacing shoes with new brake linings and/or new rear brake disc/drum.

1. Park the vehicle on a firm, level surface.

1. Do the major parking brake adjustment.

1. Do the minor parking brake adjustment.

1. Pull the parking brake lever 88 N (9 kgf, 19.8 lbf) of force while driving the vehicle for 400 m (1/4 mile).

1. Drive the vehicle for 400 m (1/4 mile) at 50 km/h (31 mph).

1. Stop the vehicle and release the parking brake for 5−10 minutes to allow the brake disc/drum to cool.

1. Repeat steps 4 through 6 three more times.

1. Check the parking brake lever adjustment.