Rear Seat Cushion Cover Replacement

NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.
- Use the handy remover set, or equivalent when prying components.

1. Remove the seat cushion.

1. Remove the screws (A) and the dampers (B), pry the clips (C) with a handy remover, then remove the seat cushion base board (D). The right seat cushion is shown; the left seat cushion is similar.

1. Release all the clips (A) from under the seat cushion, and fold back the seat cushion cover.

Right seat cushion
Left seat cushion

1. Pull back the edge of the seat cushion cover all the way around, and release the clips (A), then remove the seat cushion cover.

1. Install the cover in the reverse order of removal, and note these items:
   - To prevent wrinkles when installing a seat-back cover, make sure the material is stretched evenly over the pad before securing the hook and clips.
   - Replace any clips (A) you removed with new ones using commercially available upholstery ring pliers (B).