Steering-related Precautions Cable Reel Alignment

- Misalignment of the cable reel could cause an open in the wiring, making the SRS system and the horns inoperative. Center the cable reel whenever the following is performed.

- | Installation of the steering wheel
- | Installation of the cable reel
- | Installation of the steering column
- | Other steering-related adjustment or installation

- Do not disassemble the cable reel.
- Do not apply grease to the cable reel.
- If the cable reel shows any signs of damage, replace it with a new one. For example, if it does not rotate smoothly, replace the cable reel.