A/T differential carrier

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
A/T differential carrier | Pinion shaft contact area I.D. |  | 18.000−18.025 mm (0.708−0.710 in.) | ———
Carrier-to-pinion shaft clearance |  | 0.023−0.057 mm (0.001−0.002 in.) | 0.1 mm (0.004 in.)
Driveshaft contact area I.D. |  | 28.015−28.045 mm (1.103−1.104 in.) | ———
Carrier-to-driveshaft clearance |  | 0.035−0.086 mm (0.001−0.003 in.) | 0.12 mm (0.005 in.)
Carrier bearing starting torque (preload) | For new bearing | 2.7−3.9 N·m (28−40 kgf·cm, 24−35 lbf·in.) | Adjust
For bearing reused | 2.5−3.6 N·m (25−37 kgf·cm, 22−32 lbf·in.) | Adjust
Final driven gear backlash | References | 0.087−0.146 mm (0.003−0.006 in.) | 0.2 mm (0.008 in.)