NOTE:

- Put on gloves to protect your hands.
- Wear eye protection when removing the glass with piano wire.
- Use seat covers to avoid damaging any surfaces.
- Use glass adhesive set P/N 08C73-X0230N.

1. Remove these items:
   - Quarter pillar trim
   - Rear pillar outer trim

1. Remove the front seal (A) from the front edge of the quarter glass (B). If necessary, cut the rubber dam with a utility knife.