SRS components are located in this area. Review the SRS component locations and the precautions and procedures before performing repairs or service. NOTE:

- Use the handy remover set, or equivalent when prying components.
- When using a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend and scratch the headliner.
- Be careful not to damage the dashboard and other interior trim.

1. Remove these items:
   - Front pillar trim, both sides
   - Ceiling light
   - Front seat belt upper anchor, both sides
   - Center pillar lower trim
   - Center pillar upper trim, both sides
   - Roof end trim
   - Quarter pillar trim, both sides
   - Camera cover, with adaptive cruise control

1. From both sides, using a handy remover, release the tabs (A), then remove the sunvisor cap (B) from the bracket (C). Turn the cap, and remove it.