1. Remove the A/C condensor.

1. Remove the bolts from the A/C condenser, then remove the receiver/dryer (A), the bracket (B) and the O-rings (C).

1. Install the receiver/dryer in the reverse order of removal, and note these items:
   Replace the O-rings with new ones, and apply a thin coat of refrigarent oil (KEIHIN SP-10) before installing them. Be sure to use the correct O-rings for HFC-134a (R-134a) to avoid leakage.