Special Tools Required Mainshaft holder set 07PAB-0010001 or 07PAB-0010000

1. Remove the two bolts securing the ATF cooler inlet line brackets, ATF filter bracket bolt, line bolt, and remove the ATF cooler line/ATF filter (D) and filter brackets (E).

1. Remove the ATF cooler outlet line (F).

1. Remove the dipstick guide pipe (G).

1. Remove the A/T clutch pressure control solenoid valve A, ATF joint pipes, ATF pipe, and gasket.

1. Remove the A/T clutch pressure control solenoid valves B and C, ATF joint pipes, and gasket.

1. Remove the transmission range switch cover (H).

1. Remove the transmission range switch harness clamps (I) from the clamp bracket (J), then remove the transmission range switch (K).

1. Remove the end cover (L), dowel pins, O-rings, and end cover gasket.