1. Remove the center console.

1. Disconnect the 2P connector (A) from the cigarette lighter (B).

1. Inspect the connector terminals to be sure they are all making good contact.
   - If the terminals are bent, loose or corroded, repair them as necessary, and recheck the system.
   - If the terminals look OK, go to Step 4 .

1. Turn the ignition switch ACC (I), and check for voltage between the No. 1 and No. 2 terminals.
   - If there is no battery voltage, check for:

   - | Blown No. 9 (15 A) fuse in the under-dash fuse/relay box.
   - | Poor ground (G506).
   - | An open in the WHT/RED or BLK wire.