Removal

1. Make sure you have the anti-theft codes for the radio and the navigation system, then write down the frequencies for the radio's preset buttons.

1. Disconnect the battery negative cable, then disconnect the positive cable, and wait at least 3 minutes.

1. Remove the under-hood multi-relay box from the under-hood fuse/relay box.

1. Remove the screws (A) from the alternator and battery cable terminals.

1. Remove the two mounting bolts (B) from the under-hood fuse/relay box.

1. Remove the under cover from the under-hood fuse/relay box.

1. Disconnect the connectors from the under-hood fuse/relay box.