Installation

1. Install the VTC actuator and exhaust camshaft sprocket.
   NOTE: Installing the VTC actuator to unlock position.

1. Apply engine oil to the threads of the VTC actuator mounting bolt and exhaust camshaft mounting bolt, then install them.

1. Hold the camshaft with an open-end wrench, then tighten the bolts.

   Specified Torque
   VTC Actuator Mounting Bolt:
   113 N·m (11.5 kgf·m, 83 lbf·ft)
   Exhaust Camshaft Sprocket Mounting Bolt:
   72 N·m (7.3 kgf·m, 53 lbf·ft)

1. Holed the camshaft, and turn the VTC actuator clockwise until you hear it click.

1. Install the cam chain.