1. Tighten the bolts in sequence to the specified torque.

   Specified Torque
   8 mm Bolts: | 22 N·m (22 kgf·m, 16 lbf·ft)
   6 mm Bolts: | 12 N·m (1.2 kgf·m, 8.7 lbf·ft)
   6 mm Bolts: | (21), (22), (23)

1. Install the cam chain.

1. Install the engine wire harness connectors and wire harness clamps to the cylinder head.
   - Four injector connectors
   - Four glow plug connectors
   - Engine coolant temperature (ECT) sensor connector
   - Camshaft position (CMP) sensor connector
   - Turbocharger boost control solenoid connector

1. Install the fuel pump.

1. Install the exhaust gas recirculation (EGR) valve.

1. Install the exhaust manifold.

1. Install the intake manifold.