Rear Toe Inspection/Adjustment

1. Release the parking brake.

1. Check the toe. If it is not within the specification, go to Step 3 .

   Rear toe-in: | 2±2 mm (0.08±0.08 in.)

1. Loosen the self-locking nut (A) while holding the adjusting bolt (B).

1. Replace the self-locking nut with a new one, and lightly tighten it.
   NOTE: Always use a new self-locking nut whenever it has been loosened.

1. Turn the adjusting bolt until the toe is correct.

1. Tighten the self-locking nut to the specified torque while holding the adjusting bolt.