1. Open the sunvisor.

1. Remove the sunvisor.

1. Disconnect the 2P connector (A) from the vanity mirror light.

   Vanity mirror light: | 2 W

1. Check for continuity between the No. 1 and No. 2 terminals.
   - With the vanity mirror cover (B) opened, there should be continuity.
   - With the vanity mirror cover closed, there should be no continuity.

1. If the continuity is not as specified, replace the bulb (C) or the sunvisor.