Maintenance Schedule for Severe Conditions - European Models

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35 °C (95 °F) conditions.
- Extensive idling, or long periods of stop-and-go driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the customer's vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule.

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200 | 220 | 240
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0 | 137.5 | 150.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120 | 132 | 144
Replace engine oil | Every 10,000 km (6,250 miles) or 6 months
Replace engine oil filter | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Inspect front and rear brakes

- Check the brake pad and disc thickness. Check for damage or cracks front pad , front disc , rear pad , rear disc
- Check the brake linings for cracking, grazing, wear, and contamination
- Check the calipers for damage, leaks, and tightness

Every 10,000 km (6,250 miles) or 6 months
Check parking brake adjustment | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Check lights alignment Check the position of the headlights | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Test drive Check for road stability, noise, vibration, and dashboard operation | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Replace air cleaner element | Wet type | Every 20,000 km (12,500 miles)
Dry type | Every 40,000 km (25,000 miles)
Clean air cleaner element | Dry type only | Every 20,000 km (12,500 miles)
Replace spark plugs K20Z2 engine, K24A3 engine | K20Z2 engine | Every 40,000 km (25,000 miles)
K24A3 engine | Every 120,000 km (75,000 miles)
Inspect the valve clearance | Every 40,000 km (25,000 miles)
Inspect drive belt Check for cracks, damage, deflection, and tension |  | ● |  | ● |  | ● |  | ● |  | ● |  | ●
Replace dust and pollen filter When the customer drives primarily in urban areas that have high concentrations of soot in the air, under dusty conditions, or the air flow from the heating and cooling system control system become less than normal. | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Replace fuel filter |  |  |  |  |  | ● |  |  |  |  |  | ●
Inspect idle speed |  |  |  |  |  | ● |  |  |  |  |  | ●
Replace manual transmission fluid Use genuine Honda MTF | Every 60,000 km (37,500 miles) or 4 years
Replace automatic transmission fluid Use genuine Honda ATF-Z1 K20Z2 engine, K24A3 engine | At 60,000 km (37,500 miles) or 4 years, then every 40,000 km (25,000 miles) or 2 years
Replace engine coolant Use genuine Honda All Season Antifreeze/Coolant Type 2 | At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years
Replace brake fluid

- Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid
- Check that brake fluid level is between upper and lower marks on the reservoir

Every 3 years
Inspect vehicle corrosion: refer to the Body Repair Manual

- External Paintwork and panel Corrosion Check
- Under body Corrosion Check

Every year
Check expiry date for temporary repair kit bottle | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200 | 220 | 240
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0 | 137.5 | 150.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120 | 132 | 144
Visually inspect the following items:

- Check for correct installation and position, check for cracks, deterioration, rust, and leaks
- Check tightness of screws, nuts, and joints. If necessary, retighten

Tie-rod ends, steering gearbox, and boots Check rack grease and steering linkage. Check the boot for damage and leaking grease | Every 10,000 km (6,250 miles) or 6 months
Suspension components

- Check the bolts for tightness
- Check all dust cover for deterioration and damage

Driveshaft boots

- Check the boot and boot band for cracks
- Check rack grease

Brake hoses and lines (including ABS/VSA) Check the master cylinder and ABS/VSA modulator- control unit and leakage | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
All fluid levels and condition of fluids Check levels and check for leaks. If necessary, add engine coolant , MTF, ATF, brake fluid, and windshield fluid
Exhaust system Check the exhaust pipe and muffler for damage, leaks, and tightness K20Z2 engine , K24A3 engine
Fuel lines and connections Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts
Tyre condition Check for pressure, puncture, cuts, and irregular thread wear