Replacement (KQ Model)

1. Raise the front of the vehicle, and support it with safety stands in the proper locations.

1. Remove the front wheels.

1. Remove the brake hose mounting bolts (A).

1. Remove the flange bolt (B) while holding the pin (C) with a wrench being careful not to damage the pin boot, and pivot the caliper (D) up out of the way. Check the hose and pin boots for damage and deterioration.