Maintenance Schedule for Severe Conditions - Australia and New Zealand
37,000miles(3year)

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km per trip or, in freezing temperatures, driving less than 16 km per trip.
- Driving in extremely hot over 35 °C conditions.
- Extensive idling, or long periods of stop-and-go driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule.

Service at the indicated distance or time whichever comes first

| Replace air cleaner element

Use normal conditions except in dusty conditions.

| Replace Manual Transmission Fluid (MTF)

Use genuine Honda MTF.

| Replace Automatic Transmission Fluid (ATF)

Use genuine Honda ATF-Z1.

| Check lights alignment

Check the position of the headlights.

| Test drive (noise, stability, dashboard operation)

| Brake hoses and lines (including VSA lines)

Check the master cylinder and VSA modulator-control unit and leakage.

| All fluid levels and condition of fluids

Check levels and check for leaks. If necessary, add.

|  | Engine coolant
|  | MTF
|  | ATF
|  | Clutch fluid
|  | Power steering fluid
|  | Brake fluid
|  | Windshield fluid

| Exhaust system

Check the exhaust pipe and muffler for damage, leaks, and tightness.

| Fuel lines and connections

|  | Check fuel lines for loose connections, cracks, and deterioration.
|  | Retighten loose connections and replace any damaged parts.

Every 5,000 km or 6 months

| Replace engine oil

Every 10,000 km or 6 months

| Replace engine oil filter

| Check front and rear brakes

|  | Check the brake pad and disc thickness. Check for damage or cracks.
|  | Check the calipers for damage, leaks, and tightness.

| Tie-rod ends, steering gearbox, and boots

|  | Check rack grease and steering linkage.
|  | Check the boot for damage and leaking grease.

| Suspension components

|  | Check the bolts for tightness.
|  | Check all dust cover for deterioration and damage.

| Driveshaft boots

|  | Check the boot and boot band for cracks.
|  | Check rack grease.

At 200,000 km or 10 years, then every 100,000 km or 5 years

| Replace engine coolant

Use genuine Honda All Season Antifreeze/Coolant Type 2.

Every 3 years

| Replace brake fluid

|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
|  | Check that brake fluid level between the upper and lower marks on the reservoir.

Every 30,000 km (18,750 miles) or 1 year

| Replace dust and pollen filter

Every 10,000 km

| Rotate tyres (Check tyre inflation and condition at least once per month)