1. Park the vehicle on level ground, and turn the ignition switch OFF.

1. Remove the splash shield.

1. Remove the oil check bolt (A) and washer (B), check the condition of the fluid. If the transmission fluid is dirty, remove the drain plug (C) and washer (D).

1. Install the drain plug with a new washer.

1. Make sure you have the anti-theft codes for the audio and the navigation system, then write down the frequencies for the audio preset buttons.
   Disconnect the negative (−) cable first, then the positive (+) cable from the battery. Remove the battery.

1. Remove the air cleaner housing.