Mainshaft

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Mainshaft | End play |  | 0.14−0.21 mm (0.006−0.008 in.) | Adjust
Diameter of pilot bearing surface |  | 19.967−19.980 mm (0.7861−0.7866 in.) | 19.91 mm (0.784 in.)
Diameter of 4th and 5th gearsdistance collar |  | 35.987−36.000 mm (1.4168−1.4173 in.) | 35.93 mm (1.415 in.)
Diameter of ball bearing contact area (clutch housing side) |  | 28.002−28.015 mm (1.1024−1.1030 in.) | 27.95 mm (1.100 in.)
Diameter of needle bearing contact area |  | 41.984−42.000 mm (1.6529−1.6535 in.) | 41.93 mm (1.651 in.)
Diameter of 6th gear distance collar |  | 32.987−33.000 mm (1.2987−1.2992 in.) | 32.93 mm (1.296 in.)
Diameter of ball bearing contact area (transmission housing side) |  | 30.987−31.000 mm (1.2200−1.2205 in.) | 30.93 mm (1.218 in.)
Runout |  | 0.02 mm (0.001 in.) max. | 0.05 mm (0.002 in.)