Rear Suspension Stabilizer Link Replacement

1. Raise the rear of the vehicle, and support it with safety stands in the proper locations.

1. Remove the rear wheel.

1. Remove the self-locking nut (A) and flange nut (B) while holding the respective joint pin (C) with a hex wrench (D), then remove the stabilizer link (E).

1. Install the stabilizer link (A) on the stabilizer bar (B) and the trailing arm (C) with the joint pins set at the center of their range of the movement.
   NOTE: The paint mark (D) on the stabilizer link shows the down direction.

1. Install the new self-locking nut and flange nut, and lightly tighten them.
   NOTE: Use a new self-locking nut on reassembly.

1. Place a jack under the knuckle, and raise the suspension to load it with the vehicle's weight.

1. Tighten the self-locking nut (A) and flange nut (B) to the specified torque values while holding the respective joint pin (C) with a hex wrench (D).

1. Reinstall all removed parts and test-drive the vehicle.

1. After 5 minutes of driving, tighten the self-locking nut again to the specified torque.