1. Remove the roller (A), the select lock return spring (C), and the select lock cam B.

1. Install in the reverse order of removal.

1. Remove the dirt and oil from the sealing surface. Apply liquid gasket (P/N 08C70-K0234M) to the sealing surface.
   NOTE: If 5 minutes have passed after applying liquid gasket, reapply it and assemble the housings. Allow it to cure at least 20 minutes after assembly before filling the transmission with oil.