Front Subframe Alignment NOTE:

- Before removing the subframe, make reference marks on the subframe that line up with the edge of the rear bracket for reinstallation.
- When installing, align both installation reference holes in the subframe with the reference holes in the body using a screwdriver or tapered punch as a guide.
- After mounting the subframe and bracket loosely, align the reference marks with the edge of the rear bracket then tighten the bolts.