1. Remove the brake booster (A) from the engine compartment.
   - Be careful not to damage the booster surfaces and threads of the booster stud bolts.
   - Be careful not to bend or damage the brake lines.

1. Install the brake booster in the reverse order of removal, and note these items:
   - Tighten all mounting hardware to the specified torque values.
   - Use a new lock pin whenever installing.
   - After installing the brake booster and master cylinder, fill the reservoir with new brake fluid, bleed the brake system, and adjust the brake pedal height and free play.