Seat Cushion Cover

1. Remove the front seat.

1. 4-way power seat/8-way power seat: From under the seat cushion, detach the recline motor connector clip, if equipped, the side airbag connector clip and the seat heater connector clip. Release the seat cushion cover from the seat cushion frame spring, then pull the cover back, and remove the clamps.

1. Remove these items from the front seat, then remove the seat-back, manual seat, manual height adjustable seat, 4-way power seat, 8-way power seat :
   - Recline cover
   - Center cover
   - Front cover (4-way power seat/8-way power seat)

1. 4-way power seat/8-way power seat:
   Remove the seat-back, 4-way power seat, 8-way power seat.

1. Release the hook strips (A) from both sides the seat cushion.
   NOTE: 4-way power seat and 8-way power seat are shown; other seats are similar, but these seat-backs remains on.