VTC Actuator, Exhaust Camshaft Sprocket Removal/Installation

Removal

1. Remove the cam chain.

1. Hold the camshaft with an open-end wrench, then loosen the variable valve timing control (VTC) actuator mounting bolt and exhaust camshaft sprocket mounting bolt.

1. To the VTC actuator reused, do the following steps.

   -1. | Remove the intake camshaft, and seal the advance holes and retard holes in the No.1 camshaft journal with tape.
   -2. | Punch a hole in the tape over one of the advance holes.
   -3. | Apply air to the advance hole to release the lock.

1. Remove the VTC actuator and exhaust camshaft sprocket.

Installation

1. Install the VTC actuator and exhaust camshaft sprocket.
   NOTE: Installing the VTC actuator to unlock position.

1. Apply engine oil to the threads of the VTC actuator mounting bolt and exhaust camshaft mounting bolt, then install them.

1. Hold the camshaft with an open-end wrench, then tighten the bolts.

   Specified Torque
   VTC Actuator Mounting Bolt:
   113 N·m (11.5 kgf·m, 83 lbf·ft)
   Exhaust Camshaft Sprocket Mounting Bolt:
   72 N·m (7.3 kgf·m, 53 lbf·ft)

1. Holed the camshaft, and turn the VTC actuator clockwise until you hear it click.

1. Install the cam chain.