DTC P0380: Glow Plug Circuit Malfunction

1. Turn the ignition switch ON (II).

1. Clear the DTC with the HDS.

1. Do the GLOW PLUG TEST in the INSPECTION MENU with the HDS.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0380 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the glow plug control module, the glow plug and the ECM.■

1. Turn the ignition switch OFF.

1. Disconnect all glow plugs 1P connector.

1. Disconnect the glow plug control module 11P connector.

1. Check for continuity between each glow plug 1P connector terminal and body ground.

Is there continuity?

YES | - | Repair short in the wire between the glow plug and the glow plug control module, then go to Step 11 .
NO | - | Go to Step 9 .