Countershaft

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Countershaft | Diameter of needle bearing contact area (clutch housing side) |  | 43.974−43.990 mm (1.7313−1.7319 in.) | 43.92 mm (1.729 in.)
Diameter of distance collar contact area |  | 42.975−42.991 mm (1.6919−1.6926 in.) | 42.92 mm (1.690 in.)
Diameter of ball bearing contact area (transmission housing side) |  | 30.002−30.015 mm (1.1812−1.1817 in.) | 29.95 mm (1.179 in.)
Diameter of countershaft reverse gear |  | 45.934−45.950 mm (1.8084−1.8091 in.) | 45.88 mm (1.806 in.)
Runout |  | 0.02 mm (0.001 in.) max. | 0.05 mm (0.002 in.)
35 mm shim-to-bearing inner race clearance |  | 0.04−0.10 mm (0.0016−0.0039 in.) | Adjust