Cautions for the Vehicle

- All wheels of the vehicle should touch the ground.
- Make sure that the suspensions are not modified.
- Check the air pressure of all the tyres. If the pressures are uneven, inflate the tyres to the specified value.
- Do not place the wheels of the vehicle on a steel plate or a roller when performing the aiming.
- The vehicle should be empty and not be loaded when performing the aiming.

NOTE: Empty vehicle: A full fuel tank, tools and a spare tyre are present. Unload any baggage other than and the spare tyre.

- Make sure that all doors are closed when performing the aiming.
- Do not put any objects on the instrument panel.
- Make sure that there are no stains on the lens of the LKAS camera, and the interior and exterior surface of the front glass of the lens parts.
- Set the steering wheel in the straight ahead position.
- Do not operate the steering wheel after the vehicle is set in the aiming position.
- Shift the lever to the P position and apply the parking brake.
- If you are towing a trailer, unhitch the trailer.