Maintenance Schedule for Normal Conditions - EU
200,000km(10year)

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first

| Replace engine oil

| Replace engine oil filter

| Replace fuel filter

| Inspect drive belt

Look for cracks and damage, then check the position of the drive belt auto-tensioner indicator.

| Check front and rear brakes

|  | Check the brake pad and disc thickness. Check for damage or cracks.
|  | Check the calipers for damage, leaks, and tightness.

| Check parking brake adjustment

Check the parking brake operation.

| Replace dust and pollen filter

Replace every 20,000 km (12,500 miles) or 1 year when the customer drives primarily in urban areas that have high concentrations of soot in the air, under dusty conditions, or the air flow from the heating and air conditioning system becomes less than normal.

| Check lights alignment

Check the position of the headlights.

| Test drive (noise, stability, dashboard operation)

Visually inspect the following items:

|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks.
|  | Check tightness of screws, nuts, and joints. If necessary, retighten.

| Tie-rod ends, steering gearbox, andboots

|  | Check rack grease and steering linkage.
|  | Check the boot for damage and leaking grease.

| Suspension components

|  | Check the bolts for tightness.
|  | Check all dust covers for deterioration and damage.

| Driveshaft boots

|  | Check the boot and boot band for cracks.
|  | Check rack grease.

| Brake hoses and lines (including VSA lines)

Check the master cylinder and VSA modulator-control unit and leakage.

| All fluid levels and condition of fluid

Check levels and check for leaks. If necessary, add.

|  | Engine coolant
|  | MTF
|  | Clutch fluid
|  | Power steering fluid
|  | Brake fluid *2
|  | Windshield fluid *2

| Exhaust system

Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness.

| Fuel lines and connections

|  | Check fuel lines for loose connections, cracks, and deterioration.
|  | Retighten loose connections and replace any damaged parts.

| Tyre condition

Every 40,000 km (25,000 miles)

| Replace air cleaner element

Every 120,000 km (75,000 miles) or 8 years

| Replace Manual Transmission Fluid(MTF)

Use genuine Honda MTF.

Every 3 years

| Replace brake fluid

|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
|  | Check the brake fluid level is between the upper and lower marks on the reservoir.

Every year

| Inspect vehicle corrosion:

refer to the Body Repair Manual

|  | External paintwork and panel corrosion check
|  | Under body corrosion check