Maintenance Schedule for Normal Conditions - Australia and New Zealand Models
40,000km(2year)

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first

| Replace engine oil filter

| Replace air cleaner element

| Inspect the valve clearance

Check valve clearance

| Inspect drive belt

Check for cracks, damage, deflection, and tension

| Inspect front and rear brakes

|  | Check the brake pad and disc thickness. Check for damage or cracks front pad , front disc , rear pad , rear disc
|  | Check the calipers for damage, leaks, and tightness

| Check parking brake adjustment

Check the parking brake operation

| Check lights alignment

Check the position of the headlights

| Test drive

Check for road stability, noise, vibrations, and dashboard operation

Visually inspect the following items:

|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks
|  | Check tightness of screws, nuts, and joints. If necessary, retighten

| Tie-rod ends, steering gearbox, and boots

Check rack grease and steering linkage. Check the boot for damage and leaking grease

| Suspension components

|  | Check the bolts for tightness
|  | Check all dust cover for deterioration and damage

| Driveshaft boots

|  | Check the boot and boot band for cracks
|  | Check rack grease

| Brake hoses and lines (including VSA)

Check the master cylinder and VSA modulator-control unit and leakage

| All fluid levels and condition of fluids

Check levels and check for leaks. If necessary, add engine coolant , MTF, ATF, brake fluid, windshield fluid

| Exhaust system

Check the exhaust pipe and muffler for damage, leaks, and tightness

| Fuel lines and connections

Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts

Every 10,000 km (6,250 miles) or 1 year

| Replace engine oil

At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years

| Replace engine coolant

Use genuine Honda All Season Antifreeze/Coolant Type 2

At 120,000 km (75,000 miles) or 6 years, then every 80,000 km (50,000 miles) or 4 years

| Replace automatic transmission fluid

Use Honda ATF-Z1

Every 3 years

| Replace brake fluid

|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid
|  | Check that brake fluid level is between upper and lower marks on the reservoir

Every 30,000 km (18,750 miles) or 1 year

| Replace dust and pollen filter

Every 10,000 km (6,250 miles)

| Rotate tyres

Check tyre inflation and condition at least once one month