Exhaust Camshaft Gear B Replacement

1. Remove the cylinder head cover.

1. Hold the exhaust camshaft with an open-end wrench, then loosen the exhaust gear B mounting bolt.

1. Remove the camshafts.

1. Remove the exhaust camshaft gear B.

1. Install the exhaust camshaft gear B.

1. Install the camshafts.

1. Apply new engine oil to the threads and flange of the exhaust camshaft gear B mounting bolt, and install it. Hold the exhaust camshaft with an open-end wrench, then tighten the bolt.

   Specified Torque: | 78 N·m (8.0 kgf·m, 58 lbf·ft)

1. Install the cylinder head cover.